( TL19E00J54211500000FHAT00 )

Accessory Power Socket Test/Replacement

NOTE: If the cigarette lighter and accessory power socket do not work, check the No. 18 (7.5 A) fuse in the driver's under-dash fuse/relay box and ground (G503) first.

1. Remove the center console panel.

1. Disconnect the 2P connector (A) from the accessory power socket (B).

1. Inspect the connector terminals to be sure they are all making good contact.
   - If the terminals are bent, loose, or corroded, repair them as necessary and recheck the system.
   - If the terminals look OK, go to Step 4 .

1. Turn the ignition switch to ACC (I).

1. Measure the voltage between the accessory power socket 2P connector No. 1 terminal and body ground. There should be battery voltage.
   - If there is battery voltage, go to Step 6 .
   - If there is no battery voltage, check for:

   - | Blown No. 12 (20 A) fuse in the passenger's under-dash fuse/relay box.
   - | Faulty accessory power socket relay.
   - | Poor ground (G503).
   - | An open in the wire.

1. Check for continuity between the accessory power socket 2P connector No. 2 terminal and body ground. There should be continuity.
   - If there is continuity, go to Step 7 .
   - If there is no continuity, check for:

   - | Poor ground (G401), [G503].
   - | An open in the wire.

   [ ]: | RHD model