( TL19E00J26220219301KDAT00 )

Dashboard Driver's Lower Cover Removal/Installation

1. If necessary, push out the switch trim (A) to detach the clips and to release the tabs (B), then remove the trim from the driver's dashboard lower cover (C).

1. Install the cover in the reverse order of removal, and note these items:
   - Make sure each connector is plugged in properly.
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips into place securely.