( TL19E1AE34116300000BAAT00 )

Clutch Hydraulic System Bleeding

NOTE:

- Do not reuse the drained fluid. Use only clean genuine Honda DOT 3 or DOT 4 Brake Fluid from an unopened container. Using a non-Honda brake fluid can cause corrosion and shorten the life of the system.
- Make sure no dirt or other foreign matter is allowed to contaminate the brake fluid.
- Do not spill brake fluid on the vehicle; it may damage the paint or plastic. If brake fluid does contact the paint or plastic, wash it off immediately with water.
- If may be necessary to limit the movement of the release fork with a block of wood to remove all the air from the system.
- Use fender covers to avoid damaging painted surfaces.

1. Make sure the brake fluid level in the clutch reservoir (A) is at the MAX (upper) level line (B).

1. Attach the one end of a clear tube to the bleeder screw (A), and put the other end into a container of brake fluid. Loosen the bleeder screw to allow air to escape from the system.

1. Make sure there is an adequate supply of fluid in the reservoir, then slowly pump the clutch pedal until no more bubbles appear at the clear tube.
   NOTE: Temporary tighten the bleeder screw when clutch pedal is returned.

1. Tighten the bleeder screw securely.

1. Refill the brake fluid in the reservoir to the MAX (upper) level line.

R20A3 engine model
K24Z3 engine model