( TL19E1AE34150200000LDAT00 )

M/T Countershaft Reassembly

1. Install the 35 mm shim (A), and new ball bearing (B) using the 40 mm inner driver handle (C), 30 mm inner bearing driver attachment (D) and a press (E).
   NOTE:
   - If necessary, replace the 35 mm shim to proper one selected in Step 16 .
   - Check the ball bearing installing direction.

1. Check the clearance between the bearing and the 35 mm shim with a feeler gauge.