( TL19E1PK771000U0029FAAT00 )

DTC Troubleshooting: U0029 (107)

DTC U0029:
F-CAN Malfunction (F-CAN BUS-OFF (PCM))
NOTE: Before you troubleshoot, record all freeze data and any on-board snapshot with the HDS, and review General Troubleshooting Information.

1. Turn the ignition switch to ON (II).

1. Clear the DTC with the HDS.

1. Check for Temporary DTCs or DTCs in the PGM-FI SYSTEM with the HDS.

Is DTC U0029 indicated in the PGM-FI SYSTEM?

YES | - | Go to the DTC U0029 troubleshooting in the PGM-FI SYSTEM; R20A3 engine model, K24Z3 engine model. ■
NO | - | Go to Step 4 .

1. Check for Temporary DTCs or DTCs in the A/T SYSTEM with the HDS.

Is DTC U0029 indicated in the A/T SYSTEM?

YES | - | Go to Step 5 .
NO | - | Intermittent failure, the system is OK at this time. If any other Temporary DTCs or DTCs were indicated, go to the indicated DTC's troubleshooting.■

1. Update the PCM if it does not have the latest software; R20A3 engine model, K24Z3 engine model, or substitute a known-good PCM.

1. Start the engine, and wait for at least 2 minutes.

1. Check for Temporary DTCs or DTCs in the A/T SYSTEM with the HDS.

Is DTC U0029 indicated in the A/T SYSTEM?

YES | - | Check for poor connections or loose terminals at the PCM. If the PCM was updated, substitute a known-good PCM, then go to Step 6 . If the PCM was substituted, go to Step 1 .
NO | - | Go to Step 8 .

1. Monitor the OBD STATUS for U0029 in the DTCs MENU with the HDS.

Does the HDS indicate PASSED?

YES | - | If the PCM was updated, troubleshooting is complete. If the PCM was substituted, replace the original PCM; R20A3 engine model, K24Z3 engine model. If any other Temporary DTCs or DTCs were indicated in Step 7 , go to the indicated DTC's troubleshooting.■
NO | - | If the HDS indicates FAILED, check for poor connections or loose terminals at the PCM. If the PCM was updated, substitute a known-good PCM, then go to Step 6 . If the PCM was substituted, go to Step 1 . If the HDS indicates NOT COMPLETED, go to Step 6 .