( TL19E00J46166400000KDAT00 )

Rear Seat Removal/Installation

1. Pull the seat hook knobs (A) while pushing down on the seat cushion (B), to release the hooks (C).

1. Pull back the seat cushion to release the center seat belt (D) and the seat belt buckles (E) from their slits (F), and remove it.

1. Install the seat cushion in the reverse order of removal, and note these items:
   - Before attaching the seat cushion, make sure there are no twists or kinks in the seat belts.
   - When installing the seat cushion, slip the seat belt buckles through the slits in the seat cushion.