( TL19E00J34600000000CAAT00 )

Power Door Lock (Unlock)
The driver's MICU controls the door lock actuators UNLOCK operation based upon the input signals of each switch.

| Input | Output
--- | --- | ---

Driver's MICU

IG1 power supply
Transmission range switch (P)
Driver's door switch
Left [right] door switch
Left [right] door lock knob switch (UNLOCK)
Brake pedal position switch Trunk lid latch switch

Driver's door lock actuators (UNLOCK)
Door lock actuators (UNLOCK)

B-CAN

Front passenger's door switch
Right [left] rear door switch
Driver's door lock switch (UNLOCK)
Front passenger's door lock switch(UNLOCK)
Front passenger's door lock knob switch(UNLOCK)
Right [left] rear door lock knob switch (UNLOCK)

Door lock (UNLOCK) signal

[ ]: | RHD model