( TL19E1PE10400013001MAAT00 )

ATF Level Check

1. Remove the ATF dipstick and check the ATF level. It should be between the upper mark (A) and the lower mark (B).

1. If the ATF level is below the lower mark, check for fluid leaks at the transmission, the ATF cooler hoses and the line joints, and the cooler lines. If a problem is found, fix it before filling the transmission with ATF.
   NOTE: If the vehicle is driven when the ATF level is below the lower mark, one or more of these symptoms may occur:
   - Transmission damage will result.
   - Vehicle does not move in any gear.
   - Vehicle accelerates poorly, and flares when starting off in D, S, and R.
   - Vibration when the engine is idling.

1. If the level is above the upper mark, drain the ATF to proper level.
   NOTE: If the vehicle is driven when the ATF level is above the upper mark, the vehicle may creep forward while in N, or have problem shifting.