( TL19E00J26220200000KBAT00 )

Dashboard Replacement

SRS components are located in this area. Review the SRS component locations and the precautions and procedures before doing repairs or service.
NOTE:

- Put on gloves to protect your hands.
- Have an assistant help you when removing and installing the dashboard.
- Take care not to scratch the dashboard, the body and the other related parts.
- Take care not to bend the brackets.
- When removing components, use the trim tools or equivalent.
- LHD model is shown; RHD model is symmetrical.

1. Do the battery terminal disconnection procedure, then wait at least 3 minutes before beginning work.

1. Remove these items from the dashboard:
   - Driver's dashboard lower cover
   - Driver's dashboard undercover
   - Driver's outer dashboard trim
   - Center console panel
   - Center console rear trim
   - Driver's center trim
   - Passenger's dashboard trim
   - Passenger's center trim
   - Center console
   - Driver's rear ventilation duct and passenger's rear ventilation duct, with rear ventilation
   - Side pockets, both sides
   - Center holder
   - Climate control unit
   - Center pocket, without navigation system
   - Center panel, without audio system
   - Driver's dashboard side lid
   - Passenger's dashboard side lid
   - Dashboard side vents, both sides
   - Side defogger vent trim, both sides
   - Speaker lid
   - Glove box
   - Passenger's dashboard undercover
   - Gauge control module
   - Audio unit:

   - | Without navigation system
   - | With navigation system

   - Audio/navigation switch panel, with navigation system
   - Center display, without navigation system
   - Navigation display, with navigation system
   - Sunlight sensor
   - In-car temperature sensor
   - Center speaker, with premium sound system
   - Front pillar trim, both sides
   - Steering column
   - Shift lever, A/T model

Driver's side

1. Detach the switch subharness connector clip or the harness clip (A), and the harness clip (B) from the dashboard.