( TL19E00G10110249112FAAT00 )

Radiator and A/C Condenser Fan Low Speed Circuit Troubleshooting

1. Connect the radiator fan 2P connector No. 1 terminal to body ground with a jumper wire.

1. Turn the ignition switch to ON (II), then set the A/C button and fan control button ON.

Does the A/C condenser fan run at high speed?

YES | - | Go to Step 23 .
NO | - | Replace the radiator fan motor. ■

1. Set the A/C button and fan control button to OFF, then turn the ignition switch to LOCK (0).

1. Disconnect the jumper wire.

1. Remove the relay circuit board from the under-hood fuse/relay box, and test the fan control relay.

Is the relay OK?

YES | - | Go to Step 26 .
NO | - | Replace the relay circuit board.■