( TL19E00K75100081120FAAT00 )

DTC Troubleshooting: 12, 18

1. Check for continuity between LKAS control unit 26P connector No. 24 terminal and LKAS camera 10P connector No. 3 terminal.

Is there continuity?

YES | - | Check for loose terminals in the LKAS camera and LKAS control unit connectors, then repair if necessary. If all connections are OK, replace the LKAS camera and LKAS control unit as a set.■
NO | - | Repair an open in the wire between LKAS camera and LKAS control unit.■