( TL19E20A14666300000KCAT00 )

Cylinder Head Rocker Arm Assembly Installation

1. If the rocker arm assembly is disassembled, reassemble the rocker arm assembly.

1. Install the oil control orifice (A) with a new O-ring (B), then install the rocker arm assembly (C).

1. Install the lost motion assembles (D) and the lost motion holder (E).

1. Tighten each bolts two turns at a time in sequence.

   Specified Torque
   6 x 1.0 mm 15 N·m (1.5 kgf·m, 11 lbf·ft)

1. Adjust the valve clearance.

1. Install the cylinder head cover.