( TL19E00J10300000000FAAT22 )

Audio System Symptom Troubleshooting - Audio remote switch does not work properly

Audio remote switch does not work properly
NOTE:

- Check the vehicle battery condition first.
- Check the connectors for poor connections or loose terminals.

1. Test the audio remote switch.

Is the audio remote switch OK?

YES | - | Go to Step 2 .
NO | - | Replace the audio remote switch: With navigation system, Without navigation system. ■

1. Turn the ignition switch to ON (II).

1. Turn on the audio unit and check the audio unit operation (volume up, volume down, CH (UP), CH (DOWN), MODE).

Is the audio unit operation OK?

YES | - | Operation is normal.■
NO | - | Go to Step 4 .

1. Turn the ignition switch to LOCK (0).

1. Remove the audio unit:
   - With navigation system
   - Without navigation system

1. Disconnect audio unit connector A (24P).

1. Reconnect the audio remote switch, and measure the resistance between the audio unit connector A (24P) terminals No. 5 and No. 16 as specified in the table.

AUDIO REMOTE SWITCH TABLE

Button held down | VOL DOWN | VOL UP | CH (−) | CH (+) | MODE | (NONE)
Resistance | about 100 Ω | about 357 Ω | about 775 Ω | about 1.7 kΩ | about 3.7 kΩ | about 10 kΩ

Is the resistance OK?

YES | - | Go to Step 8 .
NO | - | Repair short or high resistance in the circuit between the audio unit and the audio remote switch. If the wires are OK, replace the cable reel. ■

1. Check for continuity between body ground and the terminals No. 5 and No. 16 of audio unit connector A (24P) individually.

Is there continuity?

YES | - | Repair short to body ground in the circuit between the audio unit and the audio remote switch. If the wires are OK, replace the cable reel. ■
NO | - | Substitute a known-good audio unit with navigation system , without navigation system , and recheck. If the symptom/indication goes away, replace the original audio unit with navigation system , without navigation system. ■