( TL19E3PE10400013012KBAT00 )

ATF Cooler Hose Replacement

K24Z3 Engine Model

1. Slide the ATF cooler/filter hoses (A) on the ATF filter (B) until they touch the filter housing, and secure the hoses with the clips (C) at 6−8 mm (0.24−0.31 in.) (D) from the filter housing.

1. Slide the ATF cooler/filter hoses (E) over the ATF lines (F) until the hose ends contact the bulge (G), and secure the hoses with the clips (H) at 6−8 mm (0.24−0.31 in.) (I) from the hose end.

1. Slide the ATF cooler inlet hose (J) over the ATF cooler inlet lines (K) until the hose ends contact the bulge (L), and secure the hose with the clips (M) at 6−8 mm (0.24−0.31 in.) (N) from the hose end.

1. Slide the ATF cooler outlet hose (O) with pink dot end (P) over the ATF cooler outlet line (Q) until the hose end contact bulge (R), and secure the hose with the clip (S) at 6−8 mm (0.24−0.31 in.) (T) from the hose end.

1. Slide the ATF cooler hose (A) over the ATF line (B) until the hose end contacts the bulge (C), and secure the hose with the clip (D) at 2−4 mm (0.08−0.16 in.) (E) from the hose end.

1. Slide the ATF cooler hose (F) over the ATF line (G) until the hose end contact the bulge (H), and secure the hose with the clip (I) at 6−8 mm (0.24−0.31 in.) (J) from the hose end.

1. Slide the ATF cooler hose (K) with yellow dot end (L) over the ATF cooler line (M) until the hose ends contacts the bulge (N), and secure the hose with the clip (O) at 2−4 mm (0.08−0.16 in.) (P) from the hose end.

1. Install the hose (Q) on the clamp (R) at the mark (S).

1. Slide the ATF cooler hoses (T) with blue dot end (U) over the ATF cooler lines (V) until the hose end contact bulge (W), and secure the hoses with the clips (X) at 6−8 mm (0.24−0.31 in.) (Y) from the hose end.