( TL19E20A20326428302FAAT00 )

Fuel Pump Circuit Troubleshooting

1. Measure the voltage between PGM-FI main relay 2 4P connector terminal No. 2 and body ground.

Is there battery voltage?

YES | - | Go to Step 20 .

NO

-

Except KN model: Go to Step 15 .
KN model:

- Replace the No. 9 FUEL PUMP (20 A) fuse in driver's the under-dash fuse/relay box.■
- Replace the driver's under-dash fuse/relay box. ■

1. Turn the ignition switch to LOCK (0).

1. Disconnect inertia switch 3P connector.