( TL19E00K76A000U1282FAAT00 )

DTC Troubleshooting: U1282

DTC U1282:
Passenger's MICU Lost Communication with Driver's MICU

1. Clear the DTCs with the HDS.

1. Turn the ignition switch to LOCK (0) and then back to ON (II).

1. Wait for 6 seconds or more.

1. Check for DTCs with the HDS.

Is DTC U1282 indicated?

YES | - | Go to the driver's MICU input test and perform all power, ground and communication input tests. If the tests prove OK, replace the driver's under-dash fuse/relay box.■
NO | - | Intermittent failure, the system is OK at this time. Check for loose or poor connections at driver's under-dash fuse/relay box connector P (20P) and the related units.■