( TL19E20A32200000000HBAT00 )

Engine Lubrication Symptom Troubleshooting Index

Symptom |  | Diagnostic procedure | Also check for
--- | --- | --- | ---
Excessive engine oil consumption | 1. 2. 3. 4. 5. | Verify that the engine oil filler cap, oil drain bolt, and oil filter are tight. Check for oil leaks. Check for worn valve guide(s) or worn valve seal(s). Check for damaged or worn piston ring(s). Check for damaged or worn engine internal parts (cylinder wall, pistons, etc.). |
Low oil pressure indicator (Red) does not come on with the ignition switch in ON (II) | 1. 2. | Do the low oil pressure indicator circuit troubleshooting (Open). Test the oil pressure switch. | An open in the wire between the engine control module (ECM)/powertrain control module (PCM) and the oil pressure switch

Low oil pressure indicator (Red) stays on

1.
2.
3.
4.
5.
6.
7.
8.

Check the engine oil level.
Do the low oil pressure indicator circuit troubleshooting (Short).
Test the oil pressure switch.
Check the engine oil pressure.
Check the oil filter for clogging.
Check the oil screen for clogging.
Check the relief valve.
Inspect the oil pump.

A wire shorted to ground between the ECM/PCM and the oil pressure switch

Engine oil level sensor system indication symbol comes on in the multi information display | Refer to the Fuel and Emissions general troubleshooting information. |
Low engine oil indication symbol comes on in the multi information display | Do the engine oil level sensor inspection. |