( TL19E00J26220257121KDAT00 )

Dashboard/Steering Hanger Beam Removal/Installation

1. Lift up on the dashboard (A) to release it from the guide pins (B) and the center pin (C) on the dashboard from the grommet (D) on the body. Carefully remove the dashboard through the front door opening. Take care not to scratch the body with the collar nuts on the passenger's side. LHD model is shown; RHD model is symmetrical.
   NOTE: Do not rest the dashboard on its lower center cover opening, or it may be damaged. Lay it on its front or back.