( TL19E00J54300031128FHAT00 )

Headlight Washer Switch Test/Replacement

1. Remove the driver's dashboard undercover, then remove the dashboard lower cover.

1. Disconnect the 5P [13P] connector (A) from the headlight washer switch (B).
   [ ]: With parking and back-up sensor off switch

1. Check for continuity between the No. 1 [No. 11] and No. 2 [No. 12] terminals.
   [ ]: With parking and back-up sensor off switch
   - There should be continuity when the switch is pushed.
   - There should be no continuity when the switch is released.

1. If the continuity is not as specified, replace the switch.

1. Install the switch in the reverse order of removal.