( TL19E00K791000R411XFAAT00 )

DTC Troubleshooting: 41-1x

1. Measure the resistance between the No. 36 terminal of SRS unit connector A (39P) and body ground, and between the No. 37 terminal and body ground. There should be an open circuit or at least 1 MΩ.

Is the resistance as specified?

YES | - | Go to Step 12 .
NO | - | Short to ground in the left engine compartment wire harness or dashboard wire harness; replace the faulty harness.■

1. Do the battery terminal reconnection procedure.

1. Turn the ignition switch to ON (II).