( TL19E00B20200062201KBAT00 )

Front Upper Arm Replacement

1. Install the upper arm (A), and lightly tighten the new upper arm mounting bolts (B), then connect the knuckle, and lightly tighten the castle nut (C).
   NOTE:
   - Be careful not to damage the ball joint boot when connecting the knuckle.
   - Before connecting the ball joint, degrease the threaded section and the tapered portion of the ball joint pin, the ball joint connecting hole, the threaded section and the mating surfaces of the castle nut.

1. Place a floor jack under the lower arm, and raise the suspension until the clearance between the top (D) of the upper arm ball joint and the backside of the fender cut out point (E) is 40 mm (1.6 in.), then tighten the upper arm mounting bolts to specified torque value.
   NOTE: To measure the specified clearance, temporarily remove the front inner fender.

1. Lower the floor jack.

1. Install the front damper/spring.

1. Place the floor jack under the lower arm, and raise the suspension to load it with the vehicle's weight.