( TL19E00J16166221301KBAT00 )

Rear Door Outer Handle Replacement

1. Remove the rod fastener (A) from the outer handle base (B), then replace it with a new one.

1. Install the handle in the reverse order of removal, and note these items:
   - Reinstall the outer handle holder before installing the outer handle cover.
   - Make sure the outer handle rod is connected securely.
   - Make sure the door locks operate properly.
   - Make sure the door handle works properly.
   - When reinstalling the door panel, make sure the plastic cover is installed properly and sealed around its outside perimeter to seal out water.