( TL19E00K791000R621XFAAT01 )

DTC Troubleshooting: 62-1x - With Seat Heater

1. Measure the resistance between the No. 1 terminal of the passenger's (LHD model) or driver's (RHD model) seat wire harness 2P connector and body ground. There should be 0−1.0 Ω.

Is resistance as specified?

YES | - | Faulty right side seat belt buckle switch; replace the right side seat belt buckle assembly. ■
NO | - | Open in the passenger's (LHD model) or driver's (RHD model) seat wire harness, SRS floor wire harness; replace the faulty harness.■