( TL19E00J26273413801KDAT00 )

Interior Trim Removal/Installation - Pillar Areas

1. Reinstall the rear pillar trim (A).

   -1. | Set the bottom hook (B) and the projections (C) of the trim to the rear shelf (D).

   -2.

   Place the trim over the rear pillar (E), and fit its upper clip (F) and the lower clips into the holes (G) in the rear pillar, then lightly push the trim into place.
   NOTE:
   - Make sure the side curtain airbag isn't tucked down under the clips and the ribs.
   - Apply pressure to the areas of the trim on the upper clip until these clip fittings are felt. If you push too hard, the clip will be damaged, and it will not hold the trim properly.
   - Make sure the upper clip portions of the trim don't come off the body by tugging on the trim.

1. Reinstall the rear door opening seal.