( TL19E00J54400050461KBAT00 )

Rear Window Replacement

1. With a sponge, apply a light coat of glass primer to the rear window (A) along the edge of the rubber dams (B) as shown, then lightly wipe it off with gauze or cheesecloth:
   - With the printed dots (C) on the rear window as a guide, apply the glass primer to both corner portions of the rear window.
   - Do not apply body primer to the rear window, and do not get body and glass primer sponges mixed up.
   - Never touch the primed surfaces with your hands. If you do, the adhesive may not bond to the rear window properly, causing a leak after the rear window is installed.
   - Keep water, dust, and abrasive materials away from the primed surfaces.