( TL19E20A14100012901KDAT00 )

Alternator Removal and Installation

Removal

1. Do the battery terminal disconnection procedure.

1. Remove the drive belt.

1. Disconnect the alternator connector (A) and BLK wire (B) from the alternator.

1. Remove the harness connector (C) and harness clamps (D) from the alternator.

1. Remove the alternator.

Installation

1. Install the alternator.

1. Connect the alternator connector (A) and BLK wire (B) to the alternator.

1. Install the harness connector (C) and harness clamp (D) to the alternator.

1. Install the drive belt.

1. Do the battery terminal reconnection procedure.