( TL19E00H46400055408KBAT00 )

Side Curtain Airbag Replacement

Removal
NOTE:

- Review the interior trim replacement procedure before doing repair or service.
- Removal of the side curtain airbag must be done according to Precaution and Procedures.
- The side curtain airbag system consists of many components. When the side curtain airbag has been deployed, go to Component Replacement/Inspection After Deployment, and replace all of the parts listed.

1. Do the battery terminal disconnection procedure, then wait for 3 minutes before starting work.

1. Remove the headliner.

1. Disconnect the SRS floor wire harness 2P connectors (A) from the side curtain airbags.

Removal
NOTE:

- Review the interior trim replacement procedure before doing repair or service.
- Removal of the side curtain airbag must be done according to Precaution and Procedures.
- The side curtain airbag system consists of many components. When the side curtain airbag has been deployed, go to Component Replacement/Inspection After Deployment, and replace all of the parts listed.

1. Do the battery terminal disconnection procedure, then wait for 3 minutes before starting work.

1. Remove the headliner.

1. Disconnect the SRS floor wire harness 2P connectors (A) from the side curtain airbags.

1. Remove the mounting bolts (A) and mounting bolts (B) from the bracket. Detach the clips (C), then remove the side curtain airbag (D).

1. Remove the mounting bolts (A) and mounting bolts (B) from the bracket. Detach the clips (C), then remove the side curtain airbag (D).

Installation
NOTE:

- Installation of the side curtain airbag must be done according to the Precautions and Procedures.
- If the airbag is frayed, or has any other visible damage, replace it. Do not attempt to repair an airbag.
- When you install the airbag, make sure it is not twisted, and that it is not caught between the inflator bracket by the bracket bolts.
- Make sure that the side curtain airbag inflator retainer is installed properly. Otherwise the airbag could incorrectly deploy and cause damage or injuries.
- Make sure you have the slack or no cutting and peeling. If tape has slack or cutting, and peeling side curtain airbag should be replacement.

1. Place the side curtain airbag assembly on the side of the roof. Tighten the side curtain airbag mounting bolts (A) and mounting bolts (B).

Installation
NOTE:

- Installation of the side curtain airbag must be done according to the Precautions and Procedures.
- If the airbag is frayed, or has any other visible damage, replace it. Do not attempt to repair an airbag.
- When you install the airbag, make sure it is not twisted, and that it is not caught between the inflator bracket by the bracket bolts.
- Make sure that the side curtain airbag inflator retainer is installed properly. Otherwise the airbag could incorrectly deploy and cause damage or injuries.
- Make sure you have the slack or no cutting and peeling. If tape has slack or cutting, and peeling side curtain airbag should be replacement.

1. Place the side curtain airbag assembly on the side of the roof. Tighten the side curtain airbag mounting bolts (A) and mounting bolts (B).

1. Connect the SRS floor wire harness 2P connectors (A) to the side curtain airbags.

1. Do the battery terminal reconnection procedure.

1. Connect the HDS, and clear the DTCs.

1. After installing the side curtain airbag, confirm proper system operation: Turn the ignition switch ON (II); the SRS indicator should come on for about 6 seconds and then go off.

1. Install all removed parts.

1. Confirm proper headliner/pillar trim overlap.

1. Connect the SRS floor wire harness 2P connectors (A) to the side curtain airbags.

1. Do the battery terminal reconnection procedure.

1. Connect the HDS, and clear the DTCs.

1. After installing the side curtain airbag, confirm proper system operation: Turn the ignition switch ON (II); the SRS indicator should come on for about 6 seconds and then go off.

1. Install all removed parts.

1. Confirm proper headliner/pillar trim overlap.