( TL19E00J46166400000KDAT00 )

Rear Seat Removal/Installation

Seat-back
NOTE: Take care not to scratch the body or tear the seat covers.

1. Remove the right seat-back (A).

   -1. | Fold the right seat-back forward.
   -2. | Release the Velcro fasteners (B), and pull back the seat-back cover (C), then remove the bolts.
   -3. | Release the hooks (D) of both pivot brackets (E).

1. Remove the bolt, then remove the center pivot bracket (A).

1. If necessary, remove the bushing (B).

1. Remove the left seat-back (A).

   -1. | Fold the left seat-back forward.
   -2. | Pull the rear center seat belt (B) out through the slit (C) in the seat belt guide (D).
   -3. | Release the Velcro fastener (E), and pull back the seat-back cover (F), then remove the bolt.
   -4. | Release the hooks (G) of the pivot bracket (H).

1. Extend the rear center seat belt (A) to remove the left seat-back (B), then release the pivot shaft (C) from the center pivot bracket (D).

1. If necessary, remove the bushing (A) from the center pivot bracket (B).

1. If necessary, remove the center pivot cover (A) from the center pivot bracket (B).

1. Remove the seat side bolster.

1. Detach the harness clip (A), and remove the bolt, then remove the pivot bracket (B).

1. Install the seat-back in the reverse order of removal, and note these items:
   - Guide the belt over the front of the seat-back as you install the seat-back.
   - Before attaching the rear seat-back, make sure there are no twists or kinks in the rear center seat belt.

Seat Cushion
NOTE: Take care not to scratch the body or tear the seat covers.

1. Fold both rear seat-backs forward.

1. For some models: Pull back the front portion of the spare tyre lid, and detach the clips:
   - With temporary repair kit (TRK)/with compact spare tyre
   - With normal spare tyre

1. Remove the bolt securing the seat cushion (A) from behind the left rear seat-back (B).

1. Raise both rear seat-backs.

1. Pull the seat hook knobs (A) while pushing down on the seat cushion (B), to release the hooks (C).

1. Pull back the seat cushion to release the center seat belt (D) and the seat belt buckles (E) from their slits (F), and remove it.

1. Install the seat cushion in the reverse order of removal, and note these items:
   - Before attaching the seat cushion, make sure there are no twists or kinks in the seat belts.
   - When installing the seat cushion, slip the seat belt buckles through the slits in the seat cushion.

Seat Side Bolster
SRS components are located in this area. Review the SRS component locations and the precautions and procedures before doing repairs or service.
NOTE: Take care not to scratch the body or tear the seat covers.

1. Remove the seat cushion.

1. Remove the bolt securing the seat side bolster (A).

1. Fold the seat-back forward.

1. Lift the seat side bolster (A) up to release the hooks (B), then remove the seat side bolster.

1. Install the seat side bolster in the reverse order of removal, and note these items:
   - Guide the belts over the front of the seat side bolster as you install the bolster.
   - Before attaching the seat side bolster, make sure there are no twists or kinks in the seat belts.