( TL19E00J36100000000FAAT09 )

Navigation System Symptom Troubleshooting - Picture is missing a color or tone or is an odd color

Picture is missing a color or tone or is an odd color
NOTE:

- Check the connectors for poor connections or loose terminals.
- Make sure that the correct version are installed.
- Inspect the DVD for dirt or damage.
- Check any official Honda service website for more service information about the navigation system.
- Check the navigation screen settings for brightness, contrast, and black level, and check the color screen for map color and menu color.
- Before troubleshooting, make sure you have anti-theft codes for the audio system and the navigation system.
- After troubleshooting, enter the anti-theft codes for the audio system and the navigation system.
- Check the vehicle battery condition first.
- Check for aftermarket accessories that may interfere with the navigation system.

1. Go into the Detail Information & Settings select Monitor Check, and use RGB Color test under Monitor Check.

Are the red, green, and blue colored circles shown?

YES | - | The system is OK at this time.■
NO | - | Go to Step 2 .

1. Turn the ignition switch to LOCK (0).

1. Disconnect navigation unit connector B (32P) and the navigation display unit 28P connector.

1. Check for loose terminals at navigation unit connector B (32P) and the navigation display unit 28P connector.

Are there loose terminals?

YES | - | Repair the terminal.■
NO | - | Go to Step 5 .

1. Check for continuity between the terminals of navigation unit connector B (32P) and the navigation display unit 28P connector according to the table.

   From terminal | To terminal
   --- | ---
   Navigation unit | Navigation display unit | Navigation unit | Navigation display unit
   B3 (GRY) | 24 (BLK) | B1 (WHT) | 8 (WHT)
   B2 (RED) | 9 (RED)
   B17 (YEL) | 22 (YEL)
   B18 (BLK) | 23 (BRN)
   B19 (GRN) | 21 (BLU)

Is there continuity between any of the terminals?

YES | - | Repair short in the wire(s) between the audio unit and stereo amplifier (replace the appropriate shielded harness).■
NO | - | Go to Step 6 .