( TL19E1PE10410445001MCAT00 )

A/T End Cover Park Lever Stop Inspection and Adjustment

1. If the measurement is out of standard, select and install the appropriate park lever stop (A) from the table.

PARK LEVER STOP

Mark | Part Number | B | C
--- | --- | --- | ---
1 | 24537-PA9-003 | 11.00 mm (0.433 in.) | 11.00 mm (0.433 in.)
2 | 24538-PA9-003 | 10.80 mm (0.425 in.) | 10.65 mm (0.419 in.)
3 | 24539-PA9-003 | 10.60 mm (0.417 in.) | 10.30 mm (0.406 in.)

1. After replacing the park lever stop, make sure the distance is within tolerance.