( TL19E00D14300014701MAAT00 )

Brake Booster Inspection

Special Tools Required
Pressure gauge joint pipes, 12 x 1.0 mm
07HAK-SG00110
Pressure gauges set
07YAJ-0010410
Vacuum gauge
07YAJ-0010610
Attachments
07410-5790102
Tube joint adapter
07410-5790503
Leak Test

1. Install the vacuum gauge (A) between the brake booster and check valve.

1. Start the engine, adjust the engine speed with the accelerator pedal so that the vacuum gauge readings show 66.7 kPa (500 mmHg, 19.7 in.Hg), then stop the engine.

1. Read the vacuum gauge.
   If the vacuum reading decreases 2.7 kPa (20 mmHg, 0.8 in.Hg) or more after 30 seconds, check following parts for leaks.
   - Check valve
   - Vacuum hose, pipe
   - Seals
   - Brake booster
   - Master cylinder
   NOTE: Do not try to disassemble the brake booster. Replace the brake booster as an assembly with a new one.

Function Test

1. Install the vacuum gauge as same as the leak test.

1. Connect the oil pressure gauges (A) to the master cylinder using the attachments pressure gauge joint pipes as shown.

1. Bleed air through the valves (B).

1. Start the engine, and let it idle.

1. Have an assistant depress the brake pedal with a 98 N (10 kgf, 22 lbf) and 294 N (30 kgf, 66 lbf) of pressure measuring with a commercially available pressure gauge (A).

1. The following pressures should be observed at the pressure gauges in each vacuum.
   Except KQ model

   Vacuum booster Vacuum kPa (mmHg, in.Hg) | Brake pedal pressure N (kgf, lbf) | Master cylinder oil pressure kPa (kgf/cm 2 , psi)
   --- | --- | ---
   0 (0, 0) | 98 (10, 22) | 0 (0, 0)
   294 (30, 66) | 1,539 (15.7, 223)
   66.7 (500, 19.7) | 98 (10, 22) | 4,988 (50.9, 723)
   294 (30, 66) | 9,055 (92.3, 1,313)

   KQ model

   Vacuum booster Vacuum kPa (mmHg, in.Hg) | Brake pedal pressure N (kgf, lbf) | Master cylinder oil pressure kPa (kgf/cm 2 , psi)
   --- | --- | ---
   0 (0, 0) | 98 (10, 22) | 0 (0, 0)
   294 (30, 66) | 1,754 (17.9, 254)
   66.7 (500, 19.7) | 98 (10, 22) | 6,399 (65.3, 928)
   294 (30, 66) | 11,809 (120.4, 1,713)

1. Inspect the master cylinder for leaks if the readings do not fall within the limits shown above.

Booster Check Valve Test

1. Disconnect the brake booster vacuum hose (A) at the booster. The check valve (B) is built into the hose.
   NOTE: If the check valve is faulty, replace the brake booster vacuum hose/check valve as an assembly.

1. Start the engine, and let it idle. There should be vacuum available. If no vacuum is available, the check valve is not working properly. Replace the brake booster vacuum hose and check valve, and retest.

Brake Booster Pushrod Thickness (Reference) |