( TL19E00J46643420901FEAT00 )

Door Lock Actuator Test

Driver's Door Without Super Locking

1. Remove the driver's door panel.

1. Disconnect the 10P connector (A) from the actuator (B).

1. Check actuator operation by connecting power and ground according to the table. To prevent damage to the actuator, apply battery voltage only momentarily.

1. If the actuator does not operate as specified, replace it.

Front Passenger's Door Without Super Locking

1. Remove the front passenger's door panel.

1. Disconnect the 10P connector (A) from the actuator (B).

1. Check actuator operation by connecting power and ground according to the table. To prevent damage to the actuator, apply battery voltage only momentarily.

1. If the actuator does not operate as specified, replace it.

Left Rear Door Without Super Locking

1. Remove the left rear door panel.

1. Disconnect the 10P connector (A) from the actuator (B).

1. Check actuator operation by connecting power and ground according to the table. To prevent damage to the actuator, apply battery voltage only momentarily.

1. If the actuator does not operate as specified, replace it.

Right Rear Door Without Super Locking

1. Remove the right rear door panel.

1. Disconnect the 10P connector (A) from the actuator (B).

1. Check actuator operation by connecting power and ground according to the table. To prevent damage to the actuator, apply battery voltage only momentarily.

1. If the actuator does not operate as specified, replace it.

Driver's Door With Super Locking

1. Remove the driver's door panel.

1. Disconnect the 10P connector (A) from the actuator (B).

1. Check actuator operation by connecting power and ground according to the table. To prevent damage to the actuator, apply battery voltage only momentarily.

1. If the actuator does not operate as specified, replace it.

Front Passenger's Door and Left Rear Door With Super Locking

1. Remove the door panel, front passenger's, left rear door.

1. Disconnect the 10P connector (A) from the actuator (B).

1. Check actuator operation by connecting power and ground according to the table. To prevent damage to the actuator, apply battery voltage only momentarily.

1. If the actuator does not operate as specified, replace it.

Right Rear Door With Super Locking

1. Remove the right rear door panel.

1. Disconnect the 10P connector (A) from the actuator (B).

1. Check actuator operation by connecting power and ground according to the table. To prevent damage to the actuator, apply battery voltage only momentarily.

1. If the actuator does not operate as specified, replace it.