( TL19E00K791000R258XFAAT00 )

DTC Troubleshooting: 25-8x

1. Measure the voltage between the No. 2 and the No. 3 terminals of SRS unit connector B (39P) and body ground. There should be less then 0.5 V.

Is the voltage as specified?

YES | - | Faulty left side seat belt outer lap tensioner; replace the left side seat belt outer lap tensioner. ■
NO | - | Short to power in the SRS floor wire harness; replace the SRS floor wire harness.■