( TL19E00J34600000000CAAT00 )

Auto Door Locks (LOCK) (KN model)
The driver's MICU controls the door lock actuators based upon the input signals from each switch.

| Input | Output
--- | --- | ---

Driver's MICU

IG1 power supply
Transmission range switch (P) position (A/T)
Driver's door switch
Left [right] rear door switch
Trunk lid latch switch
Left [right] rear door lock knob switch (LOCK)

Door lock actuator (LOCK)

B-CAN

Front passenger's door switch
Right [left] rear door switch
Driver's door lock knob switch (LOCK)
Front passenger's door lock knob switch (LOCK)
Right [left] rear door lock knob switch (LOCK)
Vehicle speed pulse signal
Engine speed signal

Door lock (LOCK) signal

[ ]: | RHD model