( TL19E1PE10411619621NAAT00 )

A/T differential carrier

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
A/T differential carrier | Pinion shaft contact area I.D. |  | 18.000−18.025 mm (0.7087−0.7096 in.) | ———
Clearance between carrier and pinion shaft |  | 0.013−0.054 mm (0.0005−0.0021 in.) | 0.1 mm (0.004 in.)
Driveshaft contact area I.D. |  | 28.021−28.051 mm (1.1032−1.1044 in.) | ———
Clearance between carrier and driveshaft |  | 0.071−0.117 mm (0.0028−0.0046 in.) | 0.12 mm (0.005 in.)
Carrier bearing starting torque (preload) | For new bearing | 2.7−3.9 N·m (28−40 kgf·cm, 24−35 lbf·in.) | Adjust
For bearing reused | 2.5−3.6 N·m (25−37 kgf·cm, 22−32 lbf·in.) | Adjust
Final driven gear backlash | (References) | 0.086−0.142 mm (0.0034−0.0056 in.) | 0.2 mm (0.008 in.)