( TL19E00J54300065021FEAT00 )

Washer Motor Test

Windshield

1. Pull the front section of the right front inner fender back.

1. Disconnect the 2P connector (A) from the washer motor (B).

1. Test the motor by connecting battery power to the No. 2 terminal and ground to the No. 1 terminal of the washer motor. The motor should run.
   - If the motor does not run or fails to run smoothly, replace it.
   - If the motor runs smoothly, but little or no washer fluid is pumped, check for a disconnected or blocked washer hose, or a clogged washer motor outlet.

Headlight Washer

1. Pull the front section of the right front inner fender back.

1. Disconnect the 2P connector (A) from the washer motor (B).

1. Test the motor by connecting battery power to the No. 1 terminal and ground to the No. 2 terminal of the washer motor. The motor should run.
   - If the motor does not run or fails to run smoothly, replace it.
   - If the motor runs smoothly, but little or no washer fluid is pumped, check for a disconnected or blocked washer hose, or a clogged washer motor outlet.