( TL19E00R311000K5352YDAT05 )

Side Sill Outer Panel Removal

NOTE: This section explains the procedures after removal of all accessories and related parts. For accessories' and related parts' removal procedure, refer to the appropriate Shop Manual.
Mass production body welding position and number
NOTE:

- Welding symbols
  : 2-Plate spot welding/ : 3-Plate spot welding/ : 4-Plate spot welding/ : MIG plug welding/ : MIG welding L= Welding length Unit: mm (in.)
- ( ): The number of welds

Construction

- Cut and pry off the side sill outer panel, and replace it.

NOTE:

- Select the cutting positions in consideration of the side sill outer panel repair part.
- Do not damage the front pillar outer separator.

- Replace the center pillar outer separator.