( TL19E00K791000R451XFAAT00 )

DTC Troubleshooting: 45-1x

1. Measure the resistance between No. 1 terminal of SRS floor wire harness 2P connector and body ground, and between the No. 2 terminal and body ground. There should be an open circuit or at least 1 MΩ.

Is the resistance as specified?

YES | - | Go to Step 10 .
NO | - | Short to ground in the SRS floor wire harness; replace the SRS floor wire harness.■

1. Do the battery terminal reconnection procedure.

1. Turn the ignition switch to ON (II).