( TL19E20A18316600000KCAT00 )

Crankshaft/Oil Seal (Transmission End) Installation

1. Connect the CKP sensor connector (A), then install the CKP sensor cover (B).

1. M/T model: Install the flywheel, clutch disc, and pressure plate.

1. A/T model: Install the drive plate.

1. Install the transmission:
   - Manual transmission
   - Automatic transmission

1. Install the engine/transmission.
   NOTE: Whenever any crankshaft or connecting rod bearing is replaced, run the engine at idle speed until it reaches normal operating temperature, then continue to running it for about 15 minutes.