( TL19E00J46127053949KBAT00 )

Front Seat-back Cover Replacement

1. Pull the side airbag harness (A) on all types of seats, the recline motor harness (B) on the 8-way power seat, and the seat-back heater harness (C) on some types of the seats out through the loop(s) (D). Release the hooks (E), then detach the clips from under the seat-back cover (F). Release the hook strip (G), and pull the bottom of the seat-back cover back, then pull the harness(es) out through the harness hole(s) (H) in the seat-back cover. The 8-way power seats are shown; other types of the seats are similar.

Driver's seat
Passenger's seat without OPDS
Passenger's seat with OPDS on RHD model