( TL19E00J26200031201KDAT00 )

Headliner Removal/Installation

1. Install the headliner in the reverse order of removal, and note these items:
   - If the side curtain airbag has deployed, replace the headliner and removed trim pieces with new ones.
   - To prevent the side curtain airbags from deploying improperly and possibly causing injury, inspect removed pieces and replace them if they have any of these types of damage:

   - | Any crease or tears in the headliner (A)
   - | Any cracks or breakages in the grab handle (B)
   - | Any damages around the grab handle holes (C) or sunvisor holes in the headliner
   - | Any cracks in the sunvisor stay base (D)
   - | Any cracks in the sunvisor bracket cover (E)
   - | Any bends or cracks in the sunvisor stay shaft (F)
   - | Any cracks in the sunvisor base (G)
   - | Any cracks or breakages in the vanity mirror base (H)
   - | Any fastener bases (I), stiffeners (J), and clip bases (K) which have come off the headliner

   - Replace the grab handle bracket mounting 6 mm bolt with a new one if it was removed.
   - When installing a new grab handle bracket, tighten it and tab plates together with their mounting bolts securely.
   - When installing the grab handle, push on the handle against the bracket (L) until the clips (M) snap into place securely.
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Replace the removed cushion tape with new ones.
   - Check that both sides of the headliner are securely attached to the trim.
   - Make sure the headliner overlaps the trim pieces correctly.
   - When reinstalling the headliner through the front passenger's door opening, be careful not to fold or bend it. Also, be careful not to scratch the body.
   - If the map light clips are removed, replace them with new ones.
   - If the roof console screw grommets are removed or if they are damaged or stress-whitened, replace them with new ones.
   - Reinstall the roof console (N) as following procedures:

   - | Install the roof console screw grommets (O) to the console with the screws (P).
   - | If equipped, connect the navigation microphone connector (Q) or the HFT microphone connector, and/or the ultrasonic sensor connector.
   - | Set the rear hooks (R), and fit the grommets into the holes in the body, then push on the console until the grommets snap into place securely.

   - Do the battery terminal reconnection procedure.
   - Check for any DTCs that may have been set during repairs, and clear them.

Headliner
Grab handle
Sunvisor
Roof console