( TL19E00J1612672130AKBAT00 )

Front Door Outer Molding Replacement

NOTE:

- If you remove the door outer molding, replace it with a new one because it will bend during removal.
- Put on gloves to protect your hands.
- Take care not to scratch the door.
- When removing components, use the trim tools or equivalent.

1. Remove these items:
   - Tweeter cover
   - Door panel
   - Power mirror

1. Using a clip remover, detach the clip, then pull back the door weatherstrip (A), and remove the screw securing the door outer molding (B).