( TL19E00K791000R611XFAAT01 )

DTC Troubleshooting: 61-1x - With Seat Heater

1. Measure the voltage between the No. 19 terminal of SRS unit connector B (39P) and body ground. There should be more than 10 V.

Is the voltage as specified?

YES | - | Go to Step 12 .
NO | - | Open in the driver's (LHD model) or passenger's (RHD model) seat wire harness, SRS floor wire harness; replace the faulty harness.■

1. Turn the ignition switch to LOCK (0).