( TL19E00J00020422281FHAT00 )

Driving Position Memory Switch Test/Replacement

1. Carefully pry the driving position memory switch (A) out from the door panel.

1. Disconnect the 7P connector (B) from the switch.

1. Carefully pry the driving position memory switch (A) out from the door panel.

1. Disconnect the 7P connector (B) from the switch.

1. Check for continuity between the terminals in each switch position according to the table.

1. If the continuity is not as specified, replace the switch.

1. Check for continuity between the terminals in each switch position according to the table.

1. If the continuity is not as specified, replace the switch.