( TL19E1PE10411354215KDAT00 )

A/T Secondary Shaft Idler Gear Removal and Installation

Special Tools Required Bearing driver attachment 42 mm 07QAD-P0A0100 Removal Place a shaft protector (A) on the secondary shaft (B), and set a puller (C) under the idler gear (D), then remove the idler gear. |

Installation Install the idler gear (A) in the direction shown on the secondary shaft (B) using the 42 mm bearing driver attachment, and a press. |