( TL19E20A14400049251KBAT00 )

Radiator Connecting Pipe Replacement

1. Drain the engine coolant.

1. Remove the thermostat housing.

1. Remove the catalytic converter.

1. Remove the connecting pipe (A).

1. Install the connecting pipe with new O-ring (B).

1. Install the catalytic converter.

1. Install the thermostat housing.

1. Refill the radiator with engine coolant, and bleed the air from the cooling system with the heater valve open.

1. Clean up any spilled engine coolant.