( TL19E00J18535132001KBAT00 )

Hood Opener Cable Replacement

NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the body and the related parts.

1. Remove these items:
   - Front grille cover
   - Front fender trim, driver's side for some models.
   - Side sill panel, driver's side for some models
   - Front inner fender, driver's side as needed
   - Kick panel, driver's side

1. LHD model: Remove the clips securing the intake air duct cover (A), and move the cover rearward.

1. Remove the bolts, and pull the left radiator upper bracket (B) (LHD model) or the right radiator upper bracket (RHD model) up to release it from the radiator (C), then remove the bracket.
   NOTE: LHD model is shown; RHD model is symmetrical, however, the shape of the bracket is different.