( TL19E00H46200053401KBAT00 )

Front Seat Belt Replacement

1. Install the buckle in the reverse order of removal, and note these items:
   - Assemble the washers and the collar on the center anchor bolt as shown.
   - Apply medium strength liquid thread lock to the center anchor bolt before reinstallation.
   - Tighten the bolts by hand first, then tighten to specification with a torque wrench.
   - Make sure the seat belt switch connector is plugged in properly.
   - Do the battery terminal reconnection procedure.
   - Check for any DTCs that may have been set during repairs, and clear them.

Center anchor bolt installation