( TL19E00K769000Y1279FAAT00 )

DTC Troubleshooting: B1279

DTC B1279:
Headlight Switch DIMMER Position Circuit Malfunction

1. Clear the DTCs with the HDS.

1. Turn the ignition switch OFF and then back to ON (II).

1. Turn the combination light (headlight) switch ON.

1. Change the dimmer switch from low beam to high beam.

1. Turn the combination light switch OFF and then to the passing position.

1. Check for DTCs with the HDS.

Is DTC B1279 indicated?

YES | - | Go to Step 7 .
NO | - | Intermittent failure, the system is OK at this time. Check for loose or poor connections.■

1. Select LIGHTING from the BODY ELECTRICAL system select menu, then enter the DATA LIST.

1. Check each combination light switch position value with the DATA LIST menu.
   When the passing switch is operated

   Data List | Value
   --- | ---
   Headlight Switch (PASSING) | ON
   Headlight Switch (High beam) | OFF

   When the headlight switch is turned ON, and the dimmer switch changed from low beam to high beam

   Data List | Value
   --- | ---
   Headlight Switch (PASSING) | OFF
   Headlight Switch (High beam) | ON
   Headlight Switch (HEADLIGHT) | OFF

Are all data list values correct?

YES | - | Faulty driver's MICU; replace the driver's under-dash fuse/relay box. ■
NO | - | Go to Step 9 .

1. Turn the ignition switch to LOCK (0).

1. Disconnect the combination light switch 12P connector.

1. Turn the ignition switch to ON (II).

1. Select LIGHTING from the BODY ELECTRICAL system select menu, then enter the DATA LIST.

1. Check each combination light switch position value with the DATA LIST menu.
   When the combination light switch is turned OFF

   Data List | Value
   --- | ---
   Headlight Switch (PASSING) | OFF
   Headlight Switch (High beam) | OFF
   Headlight Switch (HEADLIGHT) | OFF

Are all data list values indicated OFF?

YES | - | Go to Step 17 .
NO | - | Go to Step 14 .

1. Turn the ignition switch to LOCK (0).

1. Disconnect driver's under-dash fuse/relay box connector R (24P).

1. Check for continuity between body ground and driver's under-dash fuse/relay box connector R (24P) No. 8, No. 21, and No. 22 terminals.

Is there continuity?

YES | - | Repair a short to ground in the wire.■
NO | - | Faulty driver's MICU; replace the driver's under-dash fuse/relay box. ■

1. Turn the ignition switch to LOCK (0).

1. Do the combination light switch test.

Is the combination light switch OK?

YES | - | Go to Step 19 .
NO | - | Replace the combination light switch.■

1. Disconnect driver's under-dash fuse/relay box connector R (24P).