( TL19E00J54400050461KBAT00 )

Rear Window Replacement

1. With a sponge, carefully apply a light coat of body primer to any exposed paint or metal around the flange where new adhesive will be applied. Let the primer dry for at least 10 minutes:
   - Do not apply body primer to any remaining original adhesive on the flange.
   - Be careful not to mix up the body and glass primer sponges.
   - Never touch the primed surfaces with your hands.